Media Contacts:

Nisha Brown 404.652.5080

Kim Drew 404.790.6823

January 21, 2020

**DensDefy™ Transition Membrane and Primer**

DensDefy™ Transition Membrane and Primer is a gold colored, flexible, self-adhering membrane and primer used to maintain continuity of the above-grade water-resistant barrier and air barrier at complicated transition areas of the DensElement® Barrier System. The robust adhesive bonds easily to most building substrates and allows for:

* High elongation;
* Low-temperature application;
* 12-month exposure to normal weather conditions; and
* Adhesion without primer.

DensDefy™ Transition Membrane is perfect for:

* Gaps greater than 1”;
* Transitions between dissimilar materials;
* Vertical expansion, drift, or control joints; and
* The base of rough openings with the membrane looped into the joint.

Composition: DensDefy™ Transition Membrane includes 16 mils of butyl adhesive and 9 mils of HDPP facer.

Product Availability: Nationwide, via distributor or direct.

* 6” (15 cm) 8 rolls/box
* 9” (22 cm) 4 rolls/box
* 12” (30 cm) 4 rolls/box

DensDefy™ Transition Membrane is backed by a Georgia-Pacific limited warranty.

# # #